**Description:**

**Subject: 75 LPH RO System**

**Suitable for online purification for water coolers**

* **Purification by SEDIMENT + CARBON+ PRE SEDIMENT+RO MEMBRANE.**
* **Purification capacity of 75ltr/hr with membrane 1812**
* **Fully automatic operation with auto-on and auto-off facility.**
* **ABS construction for corrosion-free life span.**

**MRP:- 35000**

**Offer Price: 32000**

|  |  |
| --- | --- |
| **Standard Warranty** | **1 year on Parts & Labor 1 year on RO Membrane 6 months on Filter Cartridges** |

**Installation free of cost**



\